Text for specification

Descrizione
Protezioni laterali per supporto profili
3p
230 mm
60Classic

Norme
IEC 61439-1:2011

Valori elettrici

Proprietà materiali
Copertura:
	temperature stability 125°C, 
	self-extinguishing in acc. to UL 94, 
	creepage resistance CTI 200,
	halogen-free

Miscellaneous 
For covering the ends of the busbars in busbar systems with 3-pole system shrouding.
Is plugged onto section holder 01 017.

Brand 
Woehner or equivalent

Cod. art.
01019000