Text for specification

Description
barramento 60 x 10
comprimento 2,40 m, estanhado
100Energy
185Power
185mm-System

Standards
IEC 61439-1:2011

Approvals
UL

Electrical data
power dissipation at full load of the item:	123,0 W

Material properties
Main body:
	Cu-ETP R300 (EN 13601), tinned

corrosion-resistant, also in aggressive environments

Miscellaneous 
Tin-plated Cu busbars considerably reduce the effort of preparing the contact points.
The Cu busbars are effective protected against aggressive media.

Brand 
Woehner or equivalent

Nº da peça
01628000