Text for specification

Description
base inferior
290 x 2400
60Classic

Standards
IEC 61439-1:2011

Electrical data

Miscellaneous 
To safeguard against touching the busbars from above, below and behind, with slotted sections that can be punched out to pass leads through.

Brand 
Woehner or equivalent

Nº da peça
01046000