Text for specification

Description
barramento de seção TCC 1600 mm²
comprimento 2,40 m, estanhado
60Classic
185mm-System
centre feed unit

Standards
IEC 61439-1:2011

Electrical data
power dissipation at full load of the item:	251,0 W

diagram current capacity (IEC) 

Miscellaneous 
Tin-plated Cu busbars considerably reduce the effort of preparing the contact points.
The Cu busbars are effective protected against aggressive media.

Brand 
Woehner or equivalent

Nº da peça
01610000