Text for specification

Description
barramento em perfil duplo T 720 mm²
comprimento 653 mm, estanhado
60Classic
185mm-System
centre feed unit

Standards
IEC 61439-1:2011

Approvals
CSA, UL

Electrical data
power dissipation at full load of the item:	49,5 W

diagram current capacity (IEC) 

Miscellaneous 
Tin-plated Cu busbars considerably reduce the effort of preparing the contact points.
The Cu busbars are effective protected against aggressive media.

Brand 
Woehner or equivalent

Nº da peça
01831000