Text for specification

Description
fusível 350 A
600 V AC, fast acting
Class J, 54x181
Accessories

Standards

Approvals
CSA, UL

Electrical data

rated current (UL):	350 A
rated voltage (UL) AC:	600 V
rated voltage (UL) DC:	300 V

SCCR:	200 kA

SCCR: DC 100 kA 

Brand 
Woehner or equivalent

Nº da peça
03226000A