Text for specification

Описание 
Защитный профиль
Перфорированный
17 x 86 x 1100
60Classic

Стандарты
IEC 61439-1:2011

Электрические данные

Miscellaneous 
To safeguard against touching the busbars from above and below, with slotted sections that can be punched out to pass leads through.

Brand 
Woehner or equivalent

Арт.
01041000