招标说明

说明
通用电流互感器模块
适用于安装在连接空间中
尺寸 1 - 3
185Power

标准
IEC 60947-1:2020
IEC 60947-3:2020 AC ratings only

电气数值
Quadron®185Power Speed:
- max. 600 A
- increase of power dissipation by 30%

Quadron®185Power, connection bottom:
- max. 630 A
- increase of power dissipation by 35%

Crito®185Power connection rail, connection bottom:
- max. 750 A
- increase of power dissipation by 28%

品牌
维纳尔或同等价值的产品

订货号
33762000A